QMS Quick Learning Activity


Traceability
Quiz
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Passing score = 80%   
Select the correct answer.
	1.
	T
	F
	ISO/IEC 17025 does not require laboratories to have calibration systems in place. 

	2.
	T
	F
	ISO Guide 34 specifies requirements for reference material producers. 

	3.
	T
	F
	Calibration laboratories do not need to establish traceability.  

	4.
	T
	F
	Calibration laboratories must issue certificates that include measurement uncertainty. 

	5.
	T
	F
	Traceability does not apply to instruments and equipment. 

	6.
	T
	F
	Traceability can be referred to as a “calibration hierarchy”. 


	7.
	T
	F
	Calibration is the comparison of two measurement devices or systems, one of known uncertainty (reference standard) and one of unknown uncertainty (test equipment).  	



8. Reference Standards include: 
	A. Hard and non-consumable items
	B. Liquid standards
	C. Consumables
	D. Proficiency testing materials



9. Reference Materials include:  
	A. Hard and non-consumable items
	B. Liquid standards
	C. Consumable
	D. A & B



10. Reference Standards should be: 
	A. Traced to SI units 
	B. Provided by a competent supplier
	C. Calibrated by an ISO/IEC 17025 accredited body that can provide traceability
	D. A & B



11. Reference Materials should be: 
	A. Traced to SI units
	B. Provided by a competent supplier
	C. Calibrated by an ISO/IEC 17025 accredited body that can provide traceability
	[bookmark: _GoBack]D. A, B & C


12. Intermediate checks need defined procedures and schedules for carrying out checks to maintain confidence in the calibration status of: 
	A. Reference Standards and Materials
	B. Primary and Working Standards
	C. Transfer Standards 
	D. All of the choices
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